Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-12-56
P. 74

    Specifications

           EJU45430                             Drive unit:
                    Specifications                Propulsion system:
           Watercraft capacity:                     Jet pump
             Maximum people on board:             Jet pump type:
               1 person                             Axial flow, single stage
           Dimensions and weight:                 Impeller rotation:
             Length:                                Counterclockwise
               2240 mm (88.2 in)                  Jet thrust nozzle angle:
             Width:                                 P1: 14.4+14.4°
               680 mm (26.8 in)                     P2: 17.3+17.3°
             Height:                            Fuel and oil:
               660 mm (26.0 in)                   Recommended fuel:
             Dry weight:                            Regular unleaded gasoline
               139 kg (306 lb)                    Minimum octane rating (PON):
           Performance:                             86
             Maximum fuel consumption:            Minimum octane rating (RON):
               29.0 L/h (7.7 US gal/h, 6.4 Imp.gal/h)  90
             Cruising range at full throttle:     Recommended engine oil:
               0.62 hour                            YAMALUBE 2-W or TC-W3 outboard motor
             Trolling speed:                        oil or equivalent
               1300 ±50 r/min
           Engine:
             Engine type:
               2-stroke
             Number of cylinders:                 Fuel mixing ratio (fuel to oil):
               2                                    50 : 1
             Engine displacement:                 Fuel tank total capacity:
               701 cm³                              18 L (4.8 US gal, 4.0 Imp.gal)
             Bore × stroke:                       Fuel tank reserve capacity:
               81.0 × 68.0 mm (3.19 × 2.68 in)      5.5 L (1.5 US gal, 1.2 Imp.gal)
             Compression ratio:
               7.2 : 1
             Lubrication system:
               Pre-mixed fuel and oil
             Cooling system:
               Water
             Starting system:
               Electric
             Ignition system:
               C.D.I.
             Spark plug (NGK):
               B7HS
             Spark plug gap:
               0.6–0.7 mm (0.024–0.028 in)
             Battery capacity:
               12 V, 19 Ah
             Charging system:
               Flywheel magneto

           67

| 69 70 71 72 73 74 75 76 77 78 79 |