Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-12-56
P. 70

    Maintenance

           EJU40831
           Periodic maintenance chart
           The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
           Yamaha dealer perform the checks in the following chart. However, maintenance may need
           to be performed more frequently depending on your operating conditions. If you have any
           questions, consult a Yamaha dealer.
           This “ ” mark indicates maintenance that you may do yourself.
           This “ ” mark indicates items to be checked and serviced by a Yamaha dealer.
                                             Initial      Thereafter every
                                              10                  100    200
                 Item          Operation     hours    50 hours   hours  hours  Page
                                                     6      12    12     24
                                                   months months months months
           Spark plugs     Check, clean, replace                                64
           Lubrication points  Lubricate                                        58
           Intermediate
           housing         Lubricate                                            65
           Fuel system     Check                                                —
                           Check                                                65
           Fuel filter
                           Check, replace                                       —
           Fuel tank       Check, clean                                         —
           Carburetor      Check, adjust                                        —
           Engine idling   Check, adjust                                        66
           speed
           Carburetor throttle   Check                                          —
           shaft
           Bilge strainer  Clean                                                —
           Impeller        Check                                                —
           Jet thrust nozzle
           angle           Check, adjust                                        —
           Handlebar pivot
           shaft           Check, adjust                                        —
           Steering friction  Check, adjust                                     —
           Steering master  Check, adjust                                       —
           Throttle cable  Check, adjust                                        —
           Choke cable     Check, adjust                                        65
           Battery         Check, charge                                        —
           Rubber coupling  Check                                               —
           Engine mount    Check                                                —
           Nuts and bolts  Check                                                —

           63

| 65 66 67 68 69 70 71 72 73 74 75 |