Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 18 - LIT-18626-12-56
P. 18

    Safety information

           EJU30831                             EJU30851
             Recommended equipment                     Hazard information
           The following items  should be carried on  z When transporting  or  storing your water-
           board your watercraft:                 craft, always turn  the fuel  cock  knob to
           z Sound-signaling device               “OFF”, otherwise gasoline may overflow
            You should carry a whistle or other sound-  from the carburetor.
            signaling device that can be used to signal
            other boats. See “Rules of the Road” for
            more information.
           z Visual distress signals
            It is recommended that a U.S. Coast Guard
            approved pyrotechnic device be stored in a
            waterproof container on your watercraft. A
            mirror can also be used as an emergency
            signal. Contact a  Yamaha  dealer or the
            U.S. Coast Guard for more information.
           z Watch                              z Never start the engine or let it run for any
            A watch is  helpful so you will know how  length of time in an enclosed area. Exhaust
            long you have been operating the water-  fumes contain carbon monoxide, a color-
            craft.                                less, odorless gas that may cause loss of
           z Towline                              consciousness and death within a short
            A towline can be used to tow a disabled  time. Always operate the watercraft in an
            watercraft in an emergency.           open area.

           11

| 13 14 15 16 17 18 19 20 21 22 23 |