Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 30 - LIT-18626-12-56
P. 30

    Control function operation

           will not start. Also, the starter motor could  zle is changed, and the direction of the water-
           be damaged. [ECJ01041]               craft is changed accordingly.

                                  1

                             START

            1 Start switch                        1 Handlebar
                                                  2 Jet thrust nozzle
           The engine will not start when the clip is re-
           moved from the engine shut-off switch.  Since the strength of the jet thrust determines
           EJU31212                             the speed and degree of a turn, throttle must
           Throttle lever
                                                always be applied when attempting a turn,
           The throttle lever increases the engine speed
                                                except at trolling speed.
           when the lever is squeezed.
                                                The angle of the jet thrust nozzle can be ad-
                                                justed to suit operator preference. (See page
                                                61 for information on adjusting the jet thrust
                                                nozzle angle.)
                                                EJU31273
                                                Steering pole
                                                The steering pole can be moved up or down
                                                to change the height of the handlebars.

            1 Throttle lever
           The throttle lever returns automatically to its
           fully closed (idle) position when released.
           EJU35933
           Steering system
           By turning the handlebars in the direction you
           wish to travel, the angle of the jet thrust noz-

           23

| 25 26 27 28 29 30 31 32 33 34 35 |