Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-56
P. 80

    Trouble recovery

           EJU34735
           Submerged watercraft
           If the watercraft is submerged or flooded with
           water, drain the bilge water from the engine
           compartment. Then, have a Yamaha dealer
           service the watercraft as soon as possible.
           (1) Remove the watercraft from the water,
              and then remove the hood.
           (2) Turn the fuel cock knob to “OFF”.
           (3) Turn the watercraft over far enough to
              drain the bilge  water from  the  engine
              compartment.  NOTICE: Turning the
              watercraft on its side with the hood
              removed could cause damage to the
              steering pole. Use two people to pro-
              vide enough support to make sure
              that the steering pole is not damaged.
              [ECJ00702]
           (4) Turn the watercraft upright again.
           (5) Have the watercraft serviced  by a
              Yamaha  dealer as soon  as possible.
              NOTICE:  Be  sure to have a  Yamaha
              dealer inspect the watercraft. Other-
              wise, serious engine damage could
              result. [ECJ00792]

           73

| 75 76 77 78 79 80 81 82 83 84 |