Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-57
P. 49

    UF3P13E0.book  Page 43  Monday, June 24, 2019  1:32 PM

                                                                     Instrument operation

                            TIP:                                  The outer numbers × 1000 r/min and display
                            “MPH” is selected as the display unit at the  segments on the meter show the engine
                            Yamaha factory.                       speed.
                            To switch the speedometer display units:
                            Start the engine, stop the engine, and then
                            push the engine stop switch 3 times, pushing
                            the switch for 0.4 seconds or more each time,
                            before the  multifunction information center
                            turns  off. The speedometer display  units
                            change.
                            To  switch the speedometer display units
                            again, repeat this procedure.
                                                                          1
                                                                   1 Tachometer
                                                                  EJU43891
                                                                  Shift indicator
                                                                  This indicator shows the  reverse  gate shift
                                                                  positions: “F” (forward), “N” (neutral), and “R”
                                                                  (reverse).  (See page 36 for shifting proce-
                                                                  dures.)
                                           1

                              1 Engine stop switch

                                                                                                  2

                                                                                                  3

                                                                                                  4
                                                                                   1
                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                               1                   4 “R” (Reverse position)
                              1 Speedometer                       EJU44010
                                                                  Trim indicator
                            EJU31464
                            Tachometer                            This indicator shows the trim angle of the jet
                            The tachometer shows the engine speed.  thrust nozzle. One of the two upper display
                                                                  segments will be shown when the trim angle
                                                                  is increased, and one of the two lower display
                                                                  segments will be shown when the trim angle
                                                                  is decreased. When the  neutral position of
                                                                  the jet thrust nozzle is selected, the middle

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |