Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 107 - LIT-18626-12-57
P. 107

    UF3P13E0.book  Page 101  Monday, June 24, 2019  1:32 PM

                                                                           Trouble recovery

                            (2) While pushing the projection  on  each  (4) While pushing both sides of the fuse box
                                lock, slide the locks outward.       cover inward, pull the cover toward the
                                                                     bow and remove it.
                             3      2                  2     3

                                                                            1

                                                            1

                              1 Electrical box cover
                              2 Lock                               1 Fuse box cover
                              3 Projection
                                                                  (5) When replacing the SCU fuse,  remove
                            (3) Remove the electrical box cover from the  the screws, and then remove the fuse.
                                electrical box and move it under the deck  Install the spare fuse,  and then  tighten
                                beam toward the stern. NOTICE: Do not  the screws.
                                attempt to forcefully remove the elec-
                                trical box cover from the watercraft.  1 23     4  5       6 7
                                Otherwise, the  electrical box cover,
                                electrical system, and engine could be
                                                                                                8
                                damaged. [ECJ02610]
                                                                                                9

                                                            1                                   8
                                                                            5  10     5
                                                                   1 Electronic throttle valve fuse
                                                                   2 Fuel pump fuse
                                                                   3 Main relay drive fuse
                                                                   4 Main fuse
                                                                   5 Spare fuse
                              1 Electrical box cover               6 Fuse puller
                                                                   7 Battery fuse
                                                                   8 Screw
                                                                   9 SCU fuse (BCU fuse)
                                                                  10 Security system fuse
                                                                  (6) When  replacing a fuse other than the
                                                                     SCU fuse, remove the  fuse  using the
                                                                     fuse puller. Install a spare fuse of the
                                                                     proper amperage.  WARNING! Do not

                                                                                                 101

| 102 103 104 105 106 107 108 109 110 111 112 |