Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-57
P. 75

    UF3P13E0.book  Page 69  Monday, June 24, 2019  1:32 PM

                                                                    Pre-operation checks

                            EJU32534                              EJU32657
                            Fire extinguisher check               Jet intake checks
                            Check that there is a full fire extinguisher on  Make sure that the jet intake is not damaged
                            board.                                or clogged with weeds or debris. If the jet in-
                                                                  take is clogged, clean it. (See page 98 for in-
                                                                  formation on the jet intake.)
                                                                  EJU43221
                                                                  Jet thrust nozzle and reverse gate check
                                                                  Check the jet thrust nozzle and reverse gate
                                                                  for damage or other problem.
                                                                  EJU44250
                                                                  Stern drain plug checks
                                                                  Loosen the stern drain plugs and  remove
                                                                  them, and then make sure that the plugs and
                                                                  O-rings on the plugs are not damaged and
                            To check  the  fire extinguisher, see the  in-  that there is no foreign material on the
                            structions supplied  by the fire extinguisher  threads or O-rings on  the plugs.  NOTICE:
                            manufacturer. Always keep the fire extin-  Before installing  the stern drain plugs,
                            guisher secured in the holder with its cover in  clean the  drain plug threads and the  O-
                            place.                                rings on the plugs to remove any foreign
                            Always carry a fire extinguisher on board. A  materials, such as dirt or sand. Otherwise,
                            fire extinguisher is not standard  equipment  the stern drain plugs could be damaged,
                            with this watercraft. If you do not have one,  allowing water to enter the engine com-
                            contact a Yamaha dealer or a fire extinguish-  partment. Check the O-rings on the stern
                            er dealer to obtain one meeting the proper  drain plugs and make sure that the plugs
                            specifications.                       are tightened securely before launching
                                                                  the  watercraft. Otherwise, water may
                              Fire extinguisher:                  flood the engine compartment and cause
                                Classification:                   the watercraft to submerge. [ECJ00363]
                                  B-1
                                Capacity:
                                  2 lb or more

                            EJU40122
                            Safety equipment check
                            Check that safety equipment meeting the ap-
                            plicable regulations is on board.
                            EJU32353
                            Hull and deck check
                            Check the hull and deck for damage or other      2
                            problem.                                         1
                                                                   1 Stern drain plug
                                                                   2 O-ring

                                                                                                   69

| 70 71 72 73 74 75 76 77 78 79 80 |