Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-57
P. 46

    UF3P13E0.book  Page 40  Monday, June 24, 2019  1:32 PM

                            Watercraft operation

                            EJU40002
                              Watercraft operation modes           Number of   Low RPM Mode   “L-MODE”
                                                                     beeps       operation   indicator
                                                                                               light
                            EJU36787
                            Low RPM Mode                                         Activated    Comes
                                                                                                on
                            The Low RPM Mode is a function that limits
                                                                                Deactivated   Goes off
                            the maximum engine speed to approximately
                            70% of the maximum engine speed in  the
                                                                  TIP:
                            normal mode.
                                                                  If the remote control transmitter is operated
                            The Low RPM Mode can only be activated
                                                                  while the multifunction information center is
                            and deactivated  by operating  the remote
                                                                  in the standby state, the center performs the
                            control transmitter that is included with this
                                                                  initial operation, and then the setting is se-
                            watercraft. (See page 30 for information on
                                                                  lected.
                            the remote control transmitter.)
                                                                  To activate the Low RPM Mode:
                                                                  Push the “L-Mode” (unlock) button on the re-
                                                                  mote control transmitter for more than 4 sec-
                                                                  onds. Once the beeper sounds three times
                                                                  and the “UNLOCK” indicator light  blinks
                                                                  three times, then comes on, the “L-MODE”
                                                                  indicator light comes on and the Low RPM
                                                                  Mode is activated.
                                                                  TIP:
                                                                  If the Low RPM Mode is activated immediate-
                              1 Remote control transmitter        ly after the information display turns off, the
                                                                  “L-MODE” indicator light will not come on.
                            TIP:
                            The Low RPM Mode can only be activated
                            when the engine is  stopped in  the  unlock
                            mode of the Yamaha Security System.
                            Activating and deactivating the Low RPM
                            Mode
                            Activation of the Low RPM Mode will be con-
                            firmed by the number of beeps when the re-
                            mote control transmitter is operated, and by
                            the “L-MODE” indicator light of the multifunc-
                            tion information center. (See page 42 for in-
                            formation on  the multifunction information
                            center.)

                            40

| 41 42 43 44 45 46 47 48 49 50 51 |