Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 100 - LIT-18626-12-57
P. 100

    UF3P13E0.book  Page 94  Monday, June 24, 2019  1:32 PM

                            Specifications

                            EJU45430                                Spark plug gap:
                                      Specifications                  0.8–0.9 mm (0.031–0.035 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 19 Ah
                                3 person                            Charging system:
                              Maximum load capacity:                  Flywheel magneto
                                240 kg (530 lb)                   Drive unit:
                            Dimensions and weight:                  Propulsion system:
                              Length:                                 Jet pump
                                3350 mm (131.9 in)                  Jet pump type:
                              Width:                                  Axial flow, single stage
                                1220 mm (48.0 in)                   Impeller rotation:
                              Height:                                 Counterclockwise
                                1190 mm (46.9 in)                   Jet thrust nozzle angle:
                              Dry weight:                             24+24 °
                                349 kg (769 lb)                     Jet thrust nozzle trim angle:
                            Performance:                              -5, -3, 0, 3, 6 °
                              Maximum fuel consumption:           Fuel and oil:
                                83.7 L/h (22.1 US gal/h, 18.4 Imp.gal/h)  Recommended fuel:
                              Cruising range at full throttle:        Premium unleaded gasoline
                                0.84 hour                           Minimum octane rating (PON):
                              Trolling speed:                         91
                                1250 ±100 r/min                     Minimum octane rating (RON):
                            Engine:                                   95
                              Engine type:                          Recommended engine oil:
                                Liquid cooled 4-stroke, DOHC          YAMALUBE 4W or 4-stroke motor oil
                              Number of cylinders:
                                4
                              Engine displacement:
                                1812 cm³
                              Bore × stroke:                        Recommended engine oil type SAE:
                                86.0 × 78.0 mm (3.39 × 3.07 in)       SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Compression ratio:                    Recommended engine oil grade API:
                                8.5 : 1                               API SJ, SL
                              Valve clearance-intake (cold):        Fuel tank total capacity:
                                0.14–0.23 mm (0.0055–0.0091 in)       70 L (18.5 US gal, 15.4 Imp.gal)
                              Valve clearance-exhaust (cold):       Engine oil quantity with oil filter replacement:
                                0.36–0.45 mm (0.0142–0.0177 in)       3.7 L (3.91 US qt, 3.26 Imp.qt)
                              Lubrication system:                   Engine oil quantity without oil filter replacement:
                                Wet sump                              3.5 L (3.70 US qt, 3.08 Imp.qt)
                              Cooling system:                       Engine oil total quantity:
                                Water                                 5.3 L (5.60 US qt, 4.66 Imp.qt)
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                LFR7A

                            94

| 95 96 97 98 99 100 101 102 103 104 105 |