Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-12-58
P. 77

    UF2W16E0.book  Page 71  Monday, June 24, 2019  1:57 PM

                                                                    Pre-operation checks

                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]

                                                             2

                                                             3

                                                             4
                                             1
                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU43400
                            Trim indicator check
                            Operate the electric trim switches and check
                            that the trim indicator shows the correct trim
                            angle of the jet thrust nozzle. (See page 38 for
                            electric trim system operation procedures.)

                                               1
                              1 Trim indicator
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.
                              Engine idling speed:
                                1300 ±100 r/min

                                                                                                   71

| 72 73 74 75 76 77 78 79 80 81 82 |