Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-12-58
P. 45

    UF2W16E0.book  Page 39  Monday, June 24, 2019  1:57 PM

                                                                      Watercraft operation

                            Vertical movement of the bow will be reduced  (2) Push the electric trim up switch or elec-
                            and the watercraft will get up on plane more  tric  trim down switch to  select  the de-
                            quickly when accelerating.               sired trim angle.
                            Bow-up positions (c) and (d)
                            The bow will go up, causing the trim angle to
                            increase.
                            There is less water resistance, therefore,
                            straight-ahead acceleration is enhanced.
                            TIP:
                            The  watercraft performance characteristics
                            according to the trim angle change depend-         1
                            ing on the operating conditions.
                                                                                    2
                                                                   1 Electric trim up switch
                                                                   2 Electric trim down switch
                              (d)                                 TIP:
                                                                   When the reverse gate moves to the neutral
                                                                   or reverse position, the jet thrust nozzle will
                                                                   automatically return to the neutral position.
                                                                   When the reverse gate moves to the for-
                              (c)                                  ward position, the jet thrust nozzle will au-
                                                                   tomatically change to the set trim angle.
                               N                                   When the engine stops, the jet thrust noz-
                              (b)                                  zle returns to the neutral position.

                              (a)

                            To change the trim angle:
                            (1) If the reverse gate is in the neutral posi-
                                tion, lightly squeeze the throttle lever so
                                that the watercraft moves forward.

                                                                                                   39

| 40 41 42 43 44 45 46 47 48 49 50 |