Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-58
P. 44

    UF2W16E0.book  Page 38  Monday, June 24, 2019  1:57 PM

                            Watercraft operation

                            TIP:                                  can be operated only when the engine is run-
                            If the RiDE lever is squeezed while the throttle  ning.
                            lever is squeezed, the  watercraft  will  slow  There are 5 positions: neutral, 2 bow-down
                            down, and once stopped, move in reverse.  positions (a) and (b), and 2 bow-up positions
                            To shift into neutral from forward:   (c) and (d).
                            (1) Release the throttle lever.
                            (2) Lightly squeeze and release the RiDE le-
                                ver. The “N” (neutral) shift indicator will
                                be displayed.

                                                                               1
                                                                                    2
                                                                   1 Electric trim up switch
                                                                   2 Electric trim down switch

                                                                          (d)
                                                                              (c)

                                                                                     (b)
                                                                                         (a)

                                             1
                              1 “N” (Neutral position)
                            TIP:                                                     (d)
                            If the RiDE lever is squeezed continuously,              (c)
                            the reverse gate will move to the reverse po-
                            sition.                                                  (b)
                            EJU43161                                                 (a)
                            Electric trim system
                            The electric trim up switch and electric trim
                                                                  Bow-down positions (a) and (b)
                            down switch are located at the left handlebar  The bow will go down, causing the trim angle
                            grip and are operated to change the vertical  to decrease.
                            angle of the jet thrust nozzle, which adjusts
                            the trim angle of the watercraft. The switches

                            38

| 39 40 41 42 43 44 45 46 47 48 49 |