Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 96 - LIT-18626-12-58
P. 96

    UF2W16E0.book  Page 90  Monday, June 24, 2019  1:57 PM

                            Maintenance

                            To install the engine cover:
                            (1) Place the engine cover in its original po-
                                sition, and then push it down.

                            (2) Install the engine cover screws.
                            (3) Securely install the seats in their original
                                positions.

                            90

| 91 92 93 94 95 96 97 98 99 100 101 |