Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-59
P. 80

    UF3Y13E0.book  Page 74  Tuesday, June 4, 2019  2:12 PM

                            Operation

                            TIP:                                  current location. (See page 35 for shift sys-
                            This model is  not equipped with  a  neutral  tem operation procedures.)
                            function.                                          1
                            Operating in reverse (EX Deluxe)
                            When the RiDE lever is squeezed, the “R” (re-
                            verse) shift indicator will be displayed and the
                            watercraft will move in reverse. (See page 35
                            for shift system operation procedures.)
                                         1

                                                                   1 “N” (Neutral position)

                              1 “R” (Reverse position)

                                                                  EJU36087
                                                                  Boarding the watercraft
                                                                  EWJ01112
                                                                      WARNING
                                                                  Be sure the operator and any passengers
                                                                  have practiced boarding from the water
                                                                  while still close to shore before riding. A
                            Make sure that there are no obstacles or peo-  person who has made many unsuccessful
                            ple behind you before shifting into reverse.  attempts to get back on the watercraft
                            TIP:                                  may become fatigued and suffer from ex-
                            This model is equipped with a function which  posure, increasing the  risk of injury and
                            limits the engine speed in reverse.   drowning.
                            Operating in neutral (EX Deluxe)
                            When the RiDE lever is squeezed lightly and  Board the watercraft in water free from
                                                                  weeds and debris and at least 60 cm (2 ft)
                            released, the “N” (neutral) shift indicator will
                                                                  deep  from the bottom of  the watercraft.
                            be displayed and the watercraft will stop in its
                                                                  NOTICE: Never run the engine in water
                                                                  that is less than 60 cm (2 ft) deep from the
                                                                  bottom of the watercraft, otherwise peb-

                            74

| 75 76 77 78 79 80 81 82 83 84 85 |