Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 92 - LIT-18626-12-59
P. 92

    UF3Y13E0.book  Page 86  Tuesday, June 4, 2019  2:12 PM

                            Care and storage

                             EX Deluxe: Shift rod (reverse gate end) and  (3) Release the hooks on the port side of the
                              ball joint                             air filter case, and remove the air filter
                                                                     case cover.

                                                                               2
                                                                                                  3
                                                                   1
                                                                                                  4
                                                                                                  5

                            TIP:
                            Disconnect the shift rod from the ball joint be-
                            fore lubricating.
                            EJU44781
                            Rustproofing
                            Rustproofing the hull, deck, and engine
                            Spray metallic parts of the hull, deck, and en-  1 Hook
                                                                   2 Air filter case cover
                            gine with a rust inhibitor such as Yamalube
                                                                   3 Fuel hose
                            Silicone Protectant & Lubricant.
                                                                   4 Holder
                            Rustproofing the internal engine compo-  5 Plastic tie
                            nents
                            Rustproof the internal  engine  components  (4) Spray a rust inhibitor such as Yamalube
                            with a rust inhibitor such as Yamalube Stor-  Stor-Rite Engine Fogging Oil into the in-
                            Rite Engine Fogging Oil.                 take opening for 3 seconds. WARNING!
                            To rustproof the internal engine components:  Do not spray flammable rust inhibitor
                            (1) Remove  the seat and  fire extinguisher  products on engine surfaces while the
                                holder. (See page 44 for seat  removal
                                and installation procedures and page 49
                                for information on  the fire extinguisher
                                holder.)
                            (2) Remove the plastic tie that is fastening
                                the fuel hose to the holder on the star-
                                board side of the air filter case.

                            86

| 87 88 89 90 91 92 93 94 95 96 97 |