Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-60
P. 67

    UF4L11E0.book  Page 61  Monday, June 24, 2019  2:27 PM

                                                                    Pre-operation checks

                            falls off, allowing the watercraft to conti-  (2) As  soon as the  engine starts running,
                            nue to run and cause an accident. [EWJ01221]  push the engine stop switch to  make
                                                                     sure that the engine stops immediately.
                                                                  (3) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                                                                     the clip from the engine shut-off switch
                                                                     to make sure that the engine stops im-
                                                                     mediately.
                                                                  EJU40102
                                                                  Storage compartment checks
                                                                  Make sure  that the storage  compartments
                                                                  are not damaged and that water has not col-
                                                                  lected in the compartments. (See page 44 for
                            EJU40692
                            Switch checks                         information on the storage compartments.)
                            ECJ01311                              EJU44670
                             NOTICE                               Fire extinguisher holder checks
                                                                  Make sure that the fire extinguisher holder is
                            Do not run the engine over 4000 r/min on
                                                                  installed  in the  correct direction and is not
                            land. Also, do not run the engine for more
                                                                  damaged. (See page  47 for information on
                            than 15 seconds without supplying water,
                                                                  the fire extinguisher holder.)
                            otherwise the engine could overheat.  EJU44620
                                                                  Fire extinguisher check
                            Check the start switch, the engine stop  Check that there is a full fire extinguisher on
                            switch, and  the engine shut-off  switch for  board.
                            proper operation. (See pages 30 to 30 for in-
                            formation on operating each switch.)
                                               1

                                                        3

                                                         4

                                           2         5            To check the fire  extinguisher, see  the  in-
                                                                  structions supplied by the fire extinguisher
                              1 Start switch
                                                                  manufacturer. Always keep the fire extin-
                              2 Engine stop switch
                                                                  guisher stored in the holder.
                              3 Engine shut-off switch
                              4 Clip                              Always carry a fire extinguisher on board. A
                              5 Engine shut-off cord (lanyard)    fire extinguisher is not  standard  equipment
                                                                  with this watercraft. If you do not have one,
                            To check the operation of the switches:
                                                                  contact a Yamaha dealer or a fire extinguish-
                            (1) Push the start switch to make sure that
                                the engine starts.

                                                                                                   61

| 62 63 64 65 66 67 68 69 70 71 72 |