Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-60
P. 66

    UF4L11E0.book  Page 60  Monday, June 24, 2019  2:27 PM

                            Pre-operation checks

                            right and left fully turned positions of the jet  lever returns automatically to its fully closed
                            thrust nozzle.                        position when released.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                                                                  EJU32664
                                                                  Engine shut-off cord (lanyard) check
                              Difference between fully turned posi-  Make sure that the engine shut-off cord (lan-
                              tions of jet thrust nozzle (distances A
                              and B):                             yard) is not damaged. If the cord is damaged,
                                Maximum 5 mm (0.20 in)            replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it
                            EJU43213                              together. The  engine  shut-off cord (lan-
                            RiDE lever checks
                                                                  yard) may not pull free when the operator
                            Operate the RiDE lever several times to make
                            sure that operation is smooth throughout the
                            whole range. Also, make sure that the RiDE

                            60

| 61 62 63 64 65 66 67 68 69 70 71 |