Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-12-60
P. 37

    UF4L11E0.book  Page 31  Monday, June 24, 2019  2:27 PM

                                                             Control function operation

                            will not start. Also, the starter motor could  in reverse. If the watercraft is moving forward,
                            be damaged. [ECJ01041]                the watercraft gradually slows down until it
                                                                  stops, and then the watercraft starts moving
                                                     1            in reverse.

                                                                                      1

                              1 Start switch
                            The engine will not start under any of the fol-
                            lowing conditions:                     1 RiDE lever
                             Clip is removed  from  the engine  shut-off  When the RiDE lever is released, it automati-
                              switch.                             cally returns to its fully closed (idle) position
                             Throttle lever is squeezed.         and the reverse gate moves to the neutral po-
                             Throttle lever is malfunctioning.   sition.
                             RiDE lever is squeezed.             EJU31262
                                                                  Steering system
                             RiDE lever is malfunctioning.
                                                                  By turning the handlebars in the direction you
                            EJU31212
                            Throttle lever                        wish to travel, the angle of the jet thrust noz-
                            The throttle lever increases the engine speed
                            when the lever is squeezed.

                                     1

                              1 Throttle lever
                            The throttle lever returns automatically to its
                            fully closed (idle) position when released.
                            EJU43342
                            RiDE lever
                            When the RiDE lever is squeezed, the reverse
                            gate lowers and the watercraft starts moving

                                                                                                   31

| 32 33 34 35 36 37 38 39 40 41 42 |