Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-60
P. 69

    UF4L11E0.book  Page 63  Monday, June 24, 2019  2:27 PM

                                                                    Pre-operation checks

                            EJU40146                              EJU43392
                            Post-launch checks                    Shift system check
                            Perform the post-launch checks in the pre-  Operate the throttle lever and RiDE lever, and
                            operation checklist while the watercraft is in  check that the watercraft moves or does not
                            the water and the engine is running.  move according to the displayed shift indica-
                            To perform the post-launch checks:    tor. (See page 34 for shift system operation
                            (1) Launch the watercraft. (See page 65 for  procedures.)  WARNING! To avoid colli-
                                information on launching the watercraft.)  sions, operate at safe speeds and keep a
                            (2) Perform the checks and make sure that  safe distance away from people, objects,
                                there are no malfunctioning items or oth-  and other watercraft. [EWJ01860]
                                er problems.                                   1
                            EJU40553                                                              2
                            Cooling water pilot outlet check
                            Make sure that water is discharged from the
                                                                                                  3
                            cooling water pilot outlet while the engine is
                            running. (See page 32 for information on the                          4
                            cooling water pilot outlet.)

                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU40172
                                                                  Engine idling speed check
                                                                  Start the engine and warm it up. Use the ta-
                                                                  chometer in the multifunction  information
                            EJU32715
                            Multifunction information center check  center to make sure  that the engine  idling
                            Make sure that the multifunction information  speed is not significantly above or below the
                            center operates properly. (See page 37 for in-  specified range.
                            formation on proper operation of the multi-
                            function information center.)           Engine idling speed:
                                                                      1500 ±100 r/min

                                                                                                   63

| 64 65 66 67 68 69 70 71 72 73 74 |