Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-12-61
P. 78

    UF3V11E0.book  Page 72  Tuesday, June 18, 2019  5:16 PM

                            Pre-operation checks

                            EJU32424                              EJU36886
                            Water separator check                 Engine oil level check
                            Make sure that no water has collected in the  Make sure that the engine oil level is between
                            water separator. If water has collected in the  the minimum and maximum level marks on
                            water separator, drain it. (See page 34 for in-  the dipstick. (See page 64 for information on
                            formation on draining the water separator.)  checking the engine oil level.)

                                                             1
                                                                                        1

                              1 Water separator                    1 Dipstick
                            EJU40182
                            Engine unit check
                            Check the exterior of the engine unit for dam-
                            age or other problem.

                                                                                          1
                                                                                          2

                                                                   1 Maximum level mark
                                                                   2 Minimum level mark
                                                                  EJU32456
                                                                  Bilge water check
                                                                  Make sure that no bilge water has collected in
                                                                  the engine compartment. If bilge water has
                                                                  collected in the engine compartment, drain it.
                                                                  (See page 66 for information on draining the
                                                                  bilge water.)
                                                                  EJU32485
                                                                  Battery checks
                                                                  Make sure  that the battery  terminals  and
                                                                  breather hose are not damaged and that the
                                                                  battery leads and breather hose are connect-
                                                                  ed properly.  WARNING!  Fire or explosion
                                                                  could result if the breather hose is dam-

                            72

| 73 74 75 76 77 78 79 80 81 82 83 |