Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-12-62
P. 53

    UF3X11E0.book  Page 47  Thursday, July 4, 2019  2:27 PM

                                                                     Instrument operation

                            EJU45141
                            Status area                           TIP:
                            The areas on the left and right sides of the  If a warning is activated or a malfunction is
                            multifunction information center that show  detected, the warning bar will be displayed
                            the watercraft information and the tachome-  instead of the tachometer number display.
                            ter at the bottom of the multifunction informa-  Shift indicator
                                                                  This indicator shows the  reverse  gate shift
                            tion center do not  respond  to touch
                                                                  positions: “F” (forward), “N” (neutral), and “R”
                            operation.
                                                                  (reverse).  (See page 35 for shifting proce-
                                  1                      5        dures.)
                                                                  Fuel level meter
                                                                  The fuel level meter shows the amount of fuel
                                                                  remaining in the fuel tank using the number of
                                                                  display segments and a percentage value.
                                                     MPH          If the amount of remaining fuel is less than
                                                                  10%, the fuel level warning will activate and
                               0                          100%    the percentage display will change to “Low”.
                                13.6V           x100       N      (See page 52 for information on the fuel level
                                                RPM
                                                                  warning.)
                               2             3             4
                                                                  TIP:
                              1 Trim setting indicator
                                                                  The accuracy of  the  fuel  level meter varies
                              2 Voltmeter
                                                                  depending on the operating conditions. Use
                              3 Tachometer
                              4 Shift indicator                   this function as a reference only.
                                                                  EJU45151
                              5 Fuel level meter
                                                                  Home screen “ ”
                            Trim setting indicator                The center display of the home screen shows
                            The position of this indicator and the trim set-  the speedometer and the indicators for the
                            ting level indicate the trim setting of the jet  operation modes. (See page 39 for informa-
                            thrust nozzle. (See page 37 for information on  tion on the functions of the various modes.)
                            the trim setting.)                    TIP:
                            Voltmeter                             If the engine speed increases while the drive
                            The voltmeter shows  the battery  voltage.
                                                                  control mode screen, setting menu screen, or
                            When the battery voltage is normal, the volt-
                                                                  engine lock screen  is  displayed, the  multi-
                            meter displays approximately 14 volts.
                            If the  battery voltage has dropped or risen
                            significantly, the battery voltage warning will
                            activate and the  voltage display will blink.
                            (See page 52 for information on the battery
                            voltage warning.)
                            Tachometer
                            The tachometer shows the engine speed us-
                            ing the large number ×100 RPM (r/min) and
                            the number of display segments.

                                                                                                   47

| 48 49 50 51 52 53 54 55 56 57 58 |