Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 10 - LIT-18626-12-62
P. 10

    UF3X11E0.book  Page 4  Thursday, July 4, 2019  2:27 PM

                            General and important labels

                            Watercraft and Outboard marine engine 2001  these standards have 65% lower emissions
                            exhaust emission standards. Engines meet-  than One Star-Low Emission engines.
                            ing these standards have 75% lower emis-
                            sions than conventional carbureted two-
                            stroke engines. These engines are equivalent
                            to the U.S. EPA’s 2006 standards for marine
                            engines.

                                                                  Four Stars - Super Ultra Low Emission
                                                                  The four-star label  identifies engines  that
                                                                  meet the Air Resources Board’s  Sterndrive
                                                                  and Inboard marine  engine 2009  exhaust
                                                                  emission standards. Personal Watercraft and
                            Two Stars - Very Low Emission         Outboard marine engines may also comply
                            The two-star label identifies  engines  that  with these standards. Engines meeting these
                            meet the Air Resources Board’s Personal  standards have 90% lower emissions than
                            Watercraft and Outboard marine engine 2004  One Star-Low Emission engines.
                            exhaust emission standards. Engines meet-
                            ing these standards have 20% lower emis-
                            sions than One Star-Low Emission engines.

                            Three Stars - Ultra Low Emission
                            The three-star label identifies engines  that
                            meet the Air Resources Board’s Personal
                            Watercraft and Outboard marine engine 2008
                            exhaust emission standards or the Sterndrive
                            and Inboard marine engine 2003-2008 ex-
                            haust emission standards. Engines meeting

                            4

| 5 6 7 8 9 10 11 12 13 14 15 |