Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 107 - LIT-18626-12-62
P. 107

    UF3X11E0.book  Page 101  Thursday, July 4, 2019  2:27 PM

                                                                                Specifications

                            EJU45430                                Spark plug (NGK):
                                      Specifications                  LFR7A
                            Watercraft capacity:                    Spark plug gap:
                              Maximum people on board:                0.8–0.9 mm (0.031–0.035 in)
                                3 person                            Battery capacity:
                              Maximum load capacity:                  12 V, 19 Ah
                                240 kg (530 lb)                     Charging system:
                            Dimensions and weight:                    Flywheel magneto
                              Length:                             Drive unit:
                                3580 mm (140.9 in)                  Propulsion system:
                              Width:                                  Jet pump
                                1270 mm (50.0 in)                   Jet pump type:
                              Height:                                 Axial flow, single stage
                                1230 mm (48.4 in)                   Impeller rotation:
                              Dry weight:                             Counterclockwise
                                371 kg (818 lb) (FX SVHO)           Jet thrust nozzle angle:
                                372 kg (820 lb) (FX Cruiser SVHO)     24+24 °
                                373 kg (822 lb) (FX Limited SVHO)   Jet thrust nozzle trim angle:
                            Performance:                              -5, -3, 0, 3, 6 °
                              Maximum fuel consumption:           Fuel and oil:
                                83.7 L/h (22.1 US gal/h, 18.4 Imp.gal/h)  Recommended fuel:
                              Cruising range at full throttle:        Premium unleaded gasoline
                                0.84 hour                           Minimum octane rating (PON):
                              Trolling speed:                         91
                                1250 ±100 r/min                     Minimum octane rating (RON):
                            Engine:                                   95
                              Engine type:                          Recommended engine oil:
                                Liquid cooled 4-stroke, DOHC          YAMALUBE 4W or 4-stroke motor oil
                              Number of cylinders:
                                4
                              Engine displacement:
                                1812 cm³
                              Bore × stroke:                        Recommended engine oil type SAE:
                                86.0 × 78.0 mm (3.39 × 3.07 in)       SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Compression ratio:                    Recommended engine oil grade API:
                                8.5 : 1                               API SJ, SL
                              Valve clearance-intake (cold):        Fuel tank total capacity:
                                0.14–0.23 mm (0.0055–0.0091 in)       70 L (18.5 US gal, 15.4 Imp.gal)
                              Valve clearance-exhaust (cold):       Engine oil quantity with oil filter replacement:
                                0.36–0.45 mm (0.0142–0.0177 in)       3.7 L (3.91 US qt, 3.26 Imp.qt)
                              Lubrication system:                   Engine oil quantity without oil filter replacement:
                                Wet sump                              3.5 L (3.70 US qt, 3.08 Imp.qt)
                              Cooling system:                       Engine oil total quantity:
                                Water                                 5.3 L (5.60 US qt, 4.66 Imp.qt)
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.

                                                                                                 101

| 102 103 104 105 106 107 108 109 110 111 112 |