Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 100 - LIT-18626-12-62
P. 100

    UF3X11E0.book  Page 94  Thursday, July 4, 2019  2:27 PM

                            Care and storage

                            Checking the battery bands            To install the battery:
                            Make  sure that  the  battery bands are not  (1) Place the battery in the battery compart-
                            damaged.                                 ment and hook the battery bands onto
                                                                     the holders.
                                                                  (2) Connect the positive (+) battery lead (red)
                                                                     to the positive (+) battery terminal.
                                                                     NOTICE: Reversal of the battery leads
                                                                     will damage the electrical parts. [ECJ00262]
                                                                  (3) Connect the negative (–)  battery lead
                                                                     (black) to the negative (–) battery termi-
                                                                     nal.
                                                                  (4) Connect the breather hose to the bat-
                                                                     tery.  WARNING! Fire or explosion
                              1 Battery band                         could result if the  breather hose is
                            To store the battery:                    damaged, obstructed, or not connect-
                            (1) Clean the battery case using fresh water.  ed properly. [EWJ00452]
                            (2) If the battery terminals are dirty or cor-  (5) Make sure that the battery is securely
                                roded, clean them using a wire brush.  held in place.

                              1 Battery terminal
                            (3) Apply water-resistant grease to the bat-
                                tery terminals.
                              Recommended water-resistant grease:
                                YAMALUBE MARINE GREASE

                            (4) Store  the battery in a cool,  dry  place.
                                NOTICE: Storing the battery in an un-
                                charged condition can cause perma-
                                nent battery damage. Check the
                                battery periodically. [ECJ00103]

                            94

| 95 96 97 98 99 100 101 102 103 104 105 |