Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-62
P. 66

    UF3X11E0.book  Page 60  Thursday, July 4, 2019  2:27 PM

                            Equipment operation

                            the stern  storage compartment while  the  To  open the removable  watertight storage
                            rope is attached to the cleat.        compartment:
                                                                  (1) Remove the rear seat. (See page 54 for
                                                                     seat  removal and installation proce-
                                                                     dures.)
                                      1
                                                                  (2) Loosen the cap and remove it.

                              1 Ski rope slot
                            EJU35175
                            Beverage holder
                            The beverage holder is located near the star-  1
                            board (right) side of the multifunction infor-
                                                                   1 Cap
                            mation center.

                                                       1

                                                                         1

                                                                   1 Removable watertight storage compart-
                              1 Beverage holder
                                                                     ment
                            Do not place any items in the beverage hold-
                                                                    Removable watertight storage compart-
                            er while riding. Otherwise, the items may fall
                                                                    ment:
                            out of the beverage holder.
                                                                      Capacity:
                            EJU37235                                    9.0 L (2.4 US gal, 2.0 Imp.gal)
                            Removable watertight storage compart-
                                                                      Load limit:
                            ment
                                                                        3.0 kg (7 lb)
                            The removable watertight storage compart-
                            ment is located under the rear seat.
                                                                  To close the removable watertight storage
                            The compartment is watertight when the cap
                                                                  compartment:
                            is closed securely.
                                                                  (1) Securely install the cap by tightening it
                                                                     until it stops.
                                                                  (2) Securely install the rear seat in its original
                                                                     position.
                            60

| 61 62 63 64 65 66 67 68 69 70 71 |