Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-12-62
P. 58

    UF3X11E0.book  Page 52  Thursday, July 4, 2019  2:27 PM

                            Instrument operation

                            start the engine again, or push the “ALARM  running, the voltage display of the voltmeter
                            MUTE” button.                         blinks.

                                                    1
                                                                                           MPH

                                                                    0                           100%
                                                                     10.8V           x100       F
                                                                                     RPM
                              1 “ALARM MUTE” button
                                                                  If the battery voltage warning  is activated,
                            TIP:                                  have the watercraft  serviced by a  Yamaha
                            If the “ALARM MUTE” button was pushed to  dealer as soon as possible.
                            stop the buzzer, the buzzer will start sound-  Check engine warning “  ”
                                                                  If a sensor malfunction or a short circuit is de-
                            ing again after 5 minutes.
                                                                  tected, the warning bar is shown instead of
                            Fuel level warning
                            If the amount of remaining fuel is less than  the tachometer value display, “  ” is shown,
                            10%, the percentage display of the fuel level  and the buzzer sounds intermittently.
                            meter changes to “Low”, and the buzzer
                            sounds intermittently.

                                                                  If the check engine warning is activated, im-
                                                                  mediately reduce the engine speed, return to
                                                                  shore, and have a Yamaha dealer check the
                                                     MPH          engine.
                                                                  TIP:
                               0                           Low
                                                                  Tap “  ” to  display a description of  the
                                13.6V           x100       F      warning in the center display.
                                                RPM
                                                                  Engine overheat warning “  ”
                            If the fuel level warning is activated, refill the  If the engine temperature rises significantly,
                            fuel tank as soon as possible. (See page 62  the warning bar is shown instead of the ta-
                            for information on filling the fuel tank.)  chometer value display, “  ” and “  ”  are
                            Battery voltage warning               shown, and the buzzer sounds continuously.
                            If the battery voltage is less than 12 volts or
                            more than 18 volts when the engine is  not

                            52

| 53 54 55 56 57 58 59 60 61 62 63 |