Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-62
P. 64

    UF3X11E0.book  Page 58  Thursday, July 4, 2019  2:27 PM

                            Equipment operation

                            To open the bow storage compartment:  To close the bow storage compartment:
                            Pull the hood latch rearward, and then lift up  Push the rear of the hood down to securely
                            the rear of the hood.                 lock it in place.

                                                      1

                              1 Hood latch
                                                                  EJU45080
                                                                  Glove compartment
                                                                  The glove compartment is located in front of
                                                                  the seat.
                                                                  To open the glove compartment:
                                                                  Unhook the glove compartment latch,  and
                                          1                       then lift up the lid.

                              1 Bow storage compartment
                                                                                              1
                              Bow storage compartment:
                                Capacity:
                                  130.0 L (34.3 US gal, 28.6 Imp.gal)
                                Load limit:
                                  5.0 kg (11 lb)
                                                                   1 Glove compartment latch

                                                                                             1

                                                                   1 Glove compartment

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |