Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-63
P. 69

    UF4E14E0.book  Page 63  Wednesday, July 17, 2019  4:21 PM

                                                                    Pre-operation checks

                            EJU31982

                            EWJ00412
                                 WARNING
                            Failure to inspect or maintain the watercraft properly increases the possibility of an ac-
                            cident or damage to the watercraft. Do not operate the watercraft if you find any prob-
                            lem. If a problem cannot be corrected by the procedures provided in this manual, have
                            the watercraft inspected by a Yamaha dealer.

                            EJU41235
                            Pre-operation checklist
                            Before using this watercraft, be sure to perform the checks in the following checklist.
                                      ITEM                         ROUTINE                   PAGE
                             PRE-LAUNCH CHECKS
                                                    Ventilate the engine compartment.
                             Engine compartment                                               65
                                                    Check inside the engine compartment for damage.
                                                    Check the fuel system for leakage.
                             Fuel system                                                      65
                                                    Check the fuel level in the fuel tank.
                             Water separator        Check the water separator for water.      66
                             Engine unit            Check the exterior of the engine unit for damage.  66
                             Engine oil level       Check the engine oil level.               66
                             Bilge water            Check the engine compartment for bilge water.  66
                             Battery                Check the battery connections and electrolyte level.  66
                             Steering system        Check the steering system for proper operation.  67
                             RiDE lever             Check the RiDE lever for proper operation.  68
                             Throttle lever         Check the throttle lever for proper operation.  68
                                                    Check the remote control transmitter for proper op-
                             Remote control transmitter                                       68
                                                    eration.
                             Engine shut-off cord (lan-  Check the engine shut-off cord (lanyard) for dam-  68
                             yard)                  age.
                                                    Check the start switch, engine stop switch, and en-
                             Switches                                                         69
                                                    gine shut-off switch for proper operation.
                                                    Check the storage compartments for damage and
                             Storage compartments                                             69
                                                    water.
                             Fire extinguisher holder,   Check the fire extinguisher holder, cover, and band   69
                             cover, and band        for damage.
                             Fire extinguisher      Check the condition of the fire extinguisher.  70
                                                    Check that safety equipment meeting the applica-
                             Safety equipment                                                 70
                                                    ble regulations is on board.
                             Hull and deck          Check the hull and deck for damage.       70
                             Jet intake             Check the jet intake for damage and clogging.  70
                             Jet thrust nozzle and re-  Check the jet thrust nozzle and reverse gate for   70
                             verse gate             damage.
                                                    Check the stern drain plugs for damage and foreign
                             Stern drain plugs                                                70
                                                    material and check that they are securely installed.

                                                                                                   63

| 64 65 66 67 68 69 70 71 72 73 74 |