Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-12-63
P. 97

    UF4E14E0.book  Page 91  Wednesday, July 17, 2019  4:21 PM

                                                                                 Maintenance

                            To install the engine cover:
                            (1) Place the engine cover in its original po-
                                sition, and then push it down.

                            (2) Install the engine cover screws.
                            (3) Securely install the seats in their original
                                positions.

                                                                                                   91

| 92 93 94 95 96 97 98 99 100 101 102 |