Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-12-63
P. 85

    UF4E14E0.book  Page 79  Wednesday, July 17, 2019  4:21 PM

                                                                                      Operation

                            Operating in neutral                  deep  from the bottom of  the watercraft.
                            When the RiDE lever is squeezed lightly and  NOTICE: Never run the engine in water
                            released, the “N” (neutral) shift indicator will  that is less than 60 cm (2 ft) deep from the
                            be displayed and the watercraft will stop in its  bottom of the watercraft, otherwise peb-
                            current location. (See page 36 for shift sys-  bles or sand could be sucked into the jet
                            tem operation procedures.)            intake, causing impeller damage and en-
                                                                  gine overheating. [ECJ00473]

                                                                               60 cm (2 ft)

                                             1
                              1 “N” (Neutral position)
                                                                  TIP:
                                                                  This watercraft is equipped with a reboarding
                                                                  step, which can be lowered and used to as-
                                                                  sist in reboarding. (See page 49 for informa-
                                                                  tion on operating the reboarding step.)
                                                                  EJU36354
                                                                  Boarding alone
                                                                  (1) From the rear of  the  watercraft,  place
                                                                     both hands on the boarding platform,
                                                                     pull yourself up, and then  grasp the
                            EJU36087                                 handgrip with one hand.
                            Boarding the watercraft
                            EWJ01112
                                 WARNING
                            Be sure the operator and any passengers
                            have practiced  boarding from the water
                            while still close to shore before riding. A
                            person who has made many unsuccessful
                            attempts to get back on  the watercraft
                            may become fatigued and suffer from ex-
                            posure, increasing the risk of injury and
                            drowning.
                            Board the watercraft  in water free from
                            weeds and debris and at least 60 cm (2 ft)

                                                                                                   79

| 80 81 82 83 84 85 86 87 88 89 90 |