Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-12-63
P. 82

    UF4E14E0.book  Page 76  Wednesday, July 17, 2019  4:21 PM

                            Operation

                            (idle) position. (See page 36 for shift system  Steering control depends on the combination
                            operation procedures.)                of handlebar position and the amount of
                                                                  throttle.
                                                                  Water sucked in through the intake grate is
                                                                  pressurized by the impeller in the jet pump.
                                                                  As the pressurized water is expelled from the
                                                                  pump through the jet thrust nozzle, it creates
                                                                  thrust to move and steer the watercraft. The
                                                                  higher the engine speed, the more thrust pro-
                                                                  duced.
                                                                  The amount of jet thrust, in addition to the po-
                                             1                    sition  of the handlebars, determines how
                              1 “F” (Forward position)
                                                                  sharply you turn.
                                                                  A. More throttle produces higher thrust, so
                                                                     the watercraft will turn more sharply.

                            EJU43423
                            Turning the watercraft
                            EWJ01783
                                                                  B. Less throttle produces lower thrust, so
                                 WARNING
                                                                     the watercraft will turn more gradually.
                             Do not release the throttle lever when
                              trying to steer  away from  objects—as
                              with other powerboats, you need throt-
                              tle to steer. A collision could result in se-
                              vere injury or death.
                             When operating at higher speeds, make
                              gradual turns or slow down before turn-
                              ing. Sharp high-speed turns may cause
                              the watercraft to slide sideways or spin,
                              throwing the operator and passenger(s)
                              overboard, which could cause an injury.
                                                                  C. Releasing  the throttle lever completely
                             Take early action to avoid collisions. The
                                                                     produces only minimum thrust. If you are
                              RiDE system is not a braking device for
                                                                     traveling  at speeds above trolling, you
                              avoiding dangerous situations.
                                                                     will have rapidly  decreasing  ability to

                            76

| 77 78 79 80 81 82 83 84 85 86 87 |