Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-63
P. 64

    UF4E14E0.book  Page 58  Wednesday, July 17, 2019  4:21 PM

                            Operation and handling requirements

                            Yamalube the best choice for your Yamaha  (3) Remove the dipstick and wipe it clean.
                            engine.

                                                                                        1

                            Checking the engine oil level
                            EWJ00341
                                 WARNING
                                                                   1 Dipstick
                            Engine oil is extremely hot immediately af-
                                                                  (4) Insert the dipstick back into the dipstick
                            ter the engine is turned off. Coming in con-
                                                                     tube  completely. Remove the  dipstick
                            tact with or getting any engine oil on your
                                                                     again and make sure that the engine oil
                            clothes could result in burns.
                                                                     level is between the minimum and maxi-
                            ECJ01002                                 mum level marks.
                             NOTICE
                            Make sure  that debris and  water  do not
                            enter the oil filler hole. Debris and water in
                            the engine oil  can cause serious engine
                            damage.
                                                                                          1
                            To check the engine oil level:
                                                                                          2
                            (1) Place the watercraft in a precisely level
                                position on land with the  engine
                                stopped. If the engine was running, allow
                                the engine oil to settle by waiting 5 min-  1 Maximum level mark
                                utes or more before checking the oil lev-  2 Minimum level mark
                                el.
                                                                  (5) If the engine oil  level  is  significantly
                            (2) Remove the seats. (See page 48 for seat
                                                                     above the maximum level mark, consult
                                removal and installation procedures.)
                                                                     a Yamaha dealer. If the engine oil level is
                                                                     below the minimum level mark, add en-
                                                                     gine oil.

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |