Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-64
P. 49

    UF4G14E0.book  Page 43  Wednesday, July 10, 2019  11:14 AM

                                                                     Instrument operation

                            EJU43760                              turn off and enter a standby state. When the
                                Multifunction information
                                                                  engine is started again, the displays return to
                                          center                  their state before the center turned off, and
                            The multifunction information center displays  then the center starts to operate normally.
                            various watercraft information.       EJU35027
                                                                  Information display
                                      1      2      3             The information display shows watercraft op-
                                                                  erating conditions.
                                                                               1     2

                                             4
                              1 “UNLOCK” indicator light (VX Deluxe /
                                VX Cruiser / VX Limited)
                              2 Information display                         3 4 5 6  7  8
                              3 “L-MODE” indicator light (VX Deluxe /   1 Tachometer
                                VX Cruiser / VX Limited)
                                                                   2 Speedometer
                              4 “WARNING” indicator light
                                                                   3 Oil pressure warning indicator
                            Multifunction information center initial op-  4 Engine overheat warning indicator
                            eration                                5 Check engine warning indicator
                            When the multifunction information center is  6 Shift indicator (VX / VX Deluxe /
                                                                     VX Cruiser / VX Limited)
                            activated, all of the display segments come
                                                                   7 Fuel level warning indicator
                            on. After 2 seconds, the warning indicators in
                                                                   8 Fuel level meter
                            the information display go off, and then the
                                                                  EJU43832
                            center starts to operate normally.    Speedometer
                            If only the multifunction information center is  The speedometer shows the watercraft
                            activated, the “WARNING” indicator light  speed against water.
                            blinks once.
                            TIP:
                            VX Deluxe / VX Cruiser /  VX Limited: The
                            “UNLOCK” indicator light also comes on as
                            part of the initial operation.
                            The  “UNLOCK” indicator light will go off
                            when the engine is started.
                            Multifunction information center standby
                            state
                            If the  multifunction information center  does           1
                            not receive any operation input within 25 sec-  1 Speedometer
                            onds after the engine stops, the center will

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |