Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 102 - LIT-18626-12-64
P. 102

    UF4G14E0.book  Page 96  Wednesday, July 10, 2019  11:14 AM

                            Specifications

                            EJU45430                                Ignition system:
                                      Specifications                  T.C.I.
                            Watercraft capacity:                    Spark plug (NGK):
                              Maximum people on board:                CR9EB
                                3 person                            Spark plug gap:
                              Maximum load capacity:                  0.7–0.8 mm (0.028–0.031 in)
                                240 kg (530 lb)                     Battery capacity:
                            Dimensions and weight:                    12 V, 19 Ah
                              Length:                               Charging system:
                                3340 mm (131.5 in) (VX-C)             Flywheel magneto
                                3350 mm (131.9 in) (VX / VX Deluxe /   Drive unit:
                                VX Cruiser / VX Limited)            Propulsion system:
                              Width:                                  Jet pump
                                1220 mm (48.0 in)                   Jet pump type:
                              Height:                                 Axial flow, single stage
                                1190 mm (46.9 in)                   Impeller rotation:
                              Dry weight:                             Counterclockwise
                                314 kg (692 lb) (VX-C)              Jet thrust nozzle angle:
                                321 kg (708 lb) (VX)                  24+24 °
                                301 kg (664 lb) (VX Deluxe)       Fuel and oil:
                                303 kg (668 lb) (VX Cruiser / VX Limited)  Recommended fuel:
                            Performance:                              Regular unleaded gasoline
                              Maximum fuel consumption:             Minimum octane rating (PON):
                                33.5 L/h (8.8 US gal/h, 7.4 Imp.gal/h)  86
                              Cruising range at full throttle:      Minimum octane rating (RON):
                                2.09 hour                             90
                              Trolling speed:                       Recommended engine oil:
                                1500 ±100 r/min                       YAMALUBE 4W or 4-stroke motor oil
                            Engine:
                              Engine type:
                                Liquid cooled 4-stroke, DOHC
                              Number of cylinders:
                                3                                   Recommended engine oil type SAE:
                              Engine displacement:                    SAE 10W-30, 10W-40, 20W-40, 20W-50
                                1049 cm³                            Recommended engine oil grade API:
                              Bore × stroke:                          API SG, SH, SJ, SL
                                82.0 × 66.2 mm (3.23 × 2.61 in)     Fuel tank total capacity:
                              Compression ratio:                      70 L (18.5 US gal, 15.4 Imp.gal)
                                11.0 : 1                            Engine oil quantity with oil filter replacement:
                              Valve clearance-intake (cold):          3.4 L (3.59 US qt, 2.99 Imp.qt)
                                0.15–0.22 mm (0.0059–0.0087 in)     Engine oil quantity without oil filter replacement:
                              Valve clearance-exhaust (cold):         3.2 L (3.38 US qt, 2.82 Imp.qt)
                                0.26–0.32 mm (0.0102–0.0126 in)     Engine oil total quantity:
                              Lubrication system:                     3.7 L (3.91 US qt, 3.26 Imp.qt)
                                Dry sump
                              Cooling system:
                                Water
                              Starting system:
                                Electric

                            96

| 97 98 99 100 101 102 103 104 105 106 107 |