Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-64
P. 47

    UF4G14E0.book  Page 41  Wednesday, July 10, 2019  11:14 AM

                                                                      Watercraft operation

                            EJU43981                                 “SET” switch. Once the beeper sounds
                            Cruise assist (VX Deluxe /
                                                                     three times quickly and the digital speed-
                            VX Cruiser / VX Limited)
                                                                     ometer display starts blinking, the cruise
                            The cruise assist is a function for maintaining
                                                                     assist is activated. When the cruise as-
                            a desired engine speed within a fixed range
                                                                     sist is activated, slowly squeeze  the
                            while operating the watercraft.
                                                                     throttle lever to keep it squeezed further
                            TIP:                                     than the position at which the cruise as-
                             The cruise assist can only be set between  sist was set; releasing the throttle lever
                              engine speeds of approximately 4000    will deactivate the cruise assist.
                              r/min and approximately 7000 r/min.
                                                                  TIP:
                             The cruise assist cannot be activated in the
                                                                  The digital speedometer display blinks con-
                              Low  RPM  Mode. (See page  38 for Low
                                                                  tinually  while the cruise assist is activated.
                              RPM Mode activation procedures.)
                                                                  Make sure that the beeper has sounded and
                            Activating and deactivating the cruise as-
                            sist                                  the  digital speedometer display  is blinking
                            Activation of  the  cruise assist will be con-  before squeezing the throttle lever to the full
                                                                  throttle position. If the speedometer display is
                            firmed by the number of beeps when the
                                                                  not blinking, the cruise assist is not activated
                            “SET” switch,  cruise assist up switch,  or
                            cruise assist down switch is pushed, and by
                            the digital speedometer display of the multi-
                            function information center. (See page 43 for
                            information on the multifunction information
                            center.)
                                                        Digital
                             Number   Cruise assist opera-
                             of beeps       tion      speedome-
                                                       ter display
                                                        Starts
                                          Activated
                                                        blinking
                                                        Stops
                                         Deactivated
                                                        blinking
                                      Set engine speed in-  Continues
                                      creases or decreases  blinking
                            TIP:
                            The beeps and the blinking digital speedom-
                            eter display also indicate the activation of the
                            no-wake mode. (See page 39 for information
                            on the no-wake mode.)
                            To activate the cruise assist:
                            (1) Operate the throttle lever until the de-
                                sired engine speed is reached.
                            (2) When the engine speed reaches the de-
                                sired cruise assist  setting, push the

                                                                                                   41

| 42 43 44 45 46 47 48 49 50 51 52 |