Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-12-64
P. 73

    UF4G14E0.book  Page 67  Wednesday, July 10, 2019  11:14 AM

                                                                    Pre-operation checks

                            ed properly.  WARNING! Fire or explosion  EJU32614
                                                                  Steering system checks
                            could result if the breather hose is dam-
                                                                  Turn the handlebars to the right and left sev-
                            aged, obstructed, or not connected prop-
                                                                  eral times  to  make sure that operation is
                            erly. [EWJ00452]
                                                                  smooth and unrestricted throughout the
                             1          2                         whole range, and that the free play is not ex-
                                                                  cessive.

                                        3

                              1 Negative (–) battery terminal: Black lead
                              2 Positive (+) battery terminal: Red lead
                              3 Breather hose
                                                                  Turn the handlebars as far as possible to the
                            Make sure  that the electrolyte level  is be-
                                                                  right and left to make sure that the jet thrust
                            tween the minimum and maximum level
                                                                  nozzle moves as the handlebars are turned,
                            marks. WARNING! Never operate the wa-
                                                                  and that there is no difference between the
                            tercraft if the battery does not have suffi-
                            cient  power to start the engine or if it
                            shows any other signs of decreased pow-
                            er. Loss of battery power may leave you
                            stranded. [EWJ01241]

                              1 Maximum level mark
                              2 Minimum level mark
                            Make sure that the battery is securely held in
                            place.

                                                                                                   67

| 68 69 70 71 72 73 74 75 76 77 78 |