Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-12-64
P. 82

    UF4G14E0.book  Page 76  Wednesday, July 10, 2019  11:14 AM

                            Operation

                            dental starting or unauthorized operation by  (idle) position. (See page 36 for shift system
                            children or others.                   operation procedures.)

                                                                                   1
                                                                   1 “F” (Forward position)
                            EJU44990
                            Operating the watercraft
                            VX-C:
                            When the engine  is  running, the watercraft
                            will move forward at trolling speed even if the
                            throttle lever is in the fully closed (idle) posi-
                            tion.

                                                                  EJU43423
                                                                  Turning the watercraft
                                                                  EWJ01783
                                                                      WARNING
                                                                   Do not release the throttle lever when
                                                                   trying to  steer away from  objects—as
                            VX / VX Deluxe / VX Cruiser / VX Limited:   with other powerboats, you need throt-
                            When the throttle lever is squeezed, the “F”  tle to steer. A collision could result in se-
                            (forward) shift indicator will be displayed and  vere injury or death.
                            the watercraft will move forward. While the   When operating at higher speeds, make
                            “F” (forward) shift indicator is displayed, the  gradual turns or slow down before turn-
                            watercraft will move forward at trolling speed  ing. Sharp high-speed turns may cause
                            even if the throttle lever is in the fully closed  the watercraft to slide sideways or spin,
                                                                   throwing the operator and passenger(s)
                                                                   overboard, which could cause an injury.
                                                                   VX / VX Deluxe / VX Cruiser / VX Limited:
                                                                   Take early action to avoid collisions. The

                            76

| 77 78 79 80 81 82 83 84 85 86 87 |