Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-64
P. 46

    UF4G14E0.book  Page 40  Wednesday, July 10, 2019  11:14 AM

                            Watercraft operation

                            craft operation or when the watercraft is in  in the fully closed (idle) position when the
                            neutral.                                 no-wake mode is activated.
                            TIP:                                  TIP:
                             The no-wake mode can only be activated  The digital speedometer display blinks con-
                              after 5 seconds have elapsed since starting  tinually while the no-wake mode is activated.
                              the engine.
                             If the no-wake mode is activated when the
                              watercraft is operating in neutral, the  re-                      1
                              verse gate will move to the forward posi-
                              tion.
                            Activating and deactivating the no-wake
                            mode
                            Activation of the no-wake mode will be con-
                            firmed by the number of beeps when the
                            “NO-WAKE MODE” switch is pushed, and by
                            the digital speedometer display of the multi-  1 “NO-WAKE MODE” switch
                            function information center. (See page 43 for
                            information on the multifunction information
                            center.)

                                                        Digital
                             Number  No-wake mode oper-
                             of beeps      ation      speedome-
                                                       ter display
                                                        Starts
                                          Activated
                                                        blinking
                                                        Stops
                                         Deactivated
                                                        blinking
                            TIP:                                  To deactivate the no-wake mode:
                            The beeps and the blinking digital speedom-  Perform one of the following operations. The
                            eter display also indicate the activation of the  beeper sounds two times quickly and the di-
                            cruise assist. (See page 41 for information on  gital speedometer display stops  blinking
                            the cruise assist.)                   when the no-wake mode is deactivated.
                            To activate the no-wake mode:          Push the “NO-WAKE MODE” switch.
                            (1) Release the throttle lever and let the en-   Squeeze the throttle lever.
                                gine speed return to idle.         Squeeze the RiDE lever.
                            (2) Push and hold the “NO-WAKE MODE”
                                                                  TIP:
                                switch.  Once the beeper sounds three
                                                                  The no-wake mode is also deactivated when
                                times quickly and “8” (when kilometers
                                                                  the engine is stopped.
                                are selected) or “5” (when miles are se-
                                lected) starts blinking in the  digital
                                speedometer display, the no-wake
                                mode is activated. Keep the throttle lever

                            40

| 41 42 43 44 45 46 47 48 49 50 51 |