Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-12-64
P. 85

    UF4G14E0.book  Page 79  Wednesday, July 10, 2019  11:14 AM

                                                                                      Operation

                             VX / VX Deluxe / VX Cruiser / VX Limited:   Operating in neutral
                              To avoid rear-end collisions while oper-  When the RiDE lever is squeezed lightly and
                              ating the watercraft,  check behind you  released, the “N” (neutral) shift indicator will
                              before using the RiDE lever to slow down  be displayed and the watercraft will stop in its
                              or stop the watercraft.             current location. (See page 36 for shift sys-
                                                                  tem operation procedures.)
                            EJU43445
                            Operating the watercraft in reverse or
                            neutral (VX / VX Deluxe / VX Cruiser /
                            VX Limited)
                            Operating in reverse
                            When the RiDE lever is squeezed, the “R” (re-
                            verse) shift indicator will be displayed and the
                            watercraft will move in reverse. (See page 36
                            for shift system operation procedures.)
                                                                                   1
                                                                   1 “N” (Neutral position)

                                             1
                              1 “R” (Reverse position)

                                                                  EJU36087
                                                                  Boarding the watercraft
                                                                  EWJ01112
                                                                      WARNING
                                                                  Be sure the operator and any passengers
                                                                  have practiced boarding from the water
                                                                  while still close to shore before riding. A
                                                                  person who has made many unsuccessful
                                                                  attempts to get back on the watercraft
                            Make sure that there are no obstacles or peo-
                                                                  may become fatigued and suffer from ex-
                            ple behind you before shifting into reverse.
                                                                  posure, increasing the  risk of injury and
                            TIP:                                  drowning.
                            This model is equipped with a function which
                                                                  Board the watercraft in water free from
                            limits the engine speed in reverse.
                                                                  weeds and debris and at least 60 cm (2 ft)

                                                                                                   79

| 80 81 82 83 84 85 86 87 88 89 90 |