Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-12-64
P. 81

    UF4G14E0.book  Page 75  Wednesday, July 10, 2019  11:14 AM

                                                                                      Operation

                                the jet intake, causing impeller dam-  engine. (See page 32 for information on
                                age and engine overheating. [ECJ00473]  operating the start switch.)

                            (3) Attach the engine shut-off cord (lanyard)  EJU32863
                                                                  Stopping the engine
                                to your left wrist, and then attach the clip
                                                                  Release the throttle lever, and then push the
                                to the engine shut-off switch. (See page
                                                                  engine stop switch (red button) to stop the
                                32 for information on operating the en-
                                                                  engine.  WARNING! You need throttle to
                                gine shut-off switch.) WARNING! Check
                                                                  steer. Shutting the engine off can cause
                                that the engine shut-off cord (lanyard)
                                                                  you to hit an obstacle you are attempting
                                is attached  correctly. If the engine
                                                                  to avoid. A collision could result in severe
                                shut-off cord (lanyard) is not attached
                                                                  injury or death. [EWJ00602]
                                correctly, it may not pull free when the
                                operator falls off, allowing the water-
                                craft to continue to run and cause an
                                accident. [EWJ00582]
                                                2
                                            1

                                                        3
                                                                  EJU32873
                                                                  Leaving the watercraft
                                                                  If leaving the watercraft, remove the clip from
                                                                  the  engine shut-off switch  to prevent acci-
                              1 Clip
                              2 Engine shut-off switch
                              3 Engine shut-off cord (lanyard)
                            (4) With the throttle lever released, push the
                                start  switch (green  button) to start  the

                                                                                                   75

| 76 77 78 79 80 81 82 83 84 85 86 |