Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-12-64
P. 74

    UF4G14E0.book  Page 68  Wednesday, July 10, 2019  11:14 AM

                            Pre-operation checks

                            right and left fully turned positions of the jet  lever returns automatically to its fully closed
                            thrust nozzle.                        position when released.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                                                                  EJU40113
                                                                  Remote control transmitter check
                              Difference between fully turned posi-  (VX Deluxe / VX Cruiser / VX Limited)
                              tions of jet thrust nozzle (distances A
                              and B):                             Make sure that the remote control transmitter
                                Maximum 5 mm (0.20 in)            operates properly. (See page 31 for Yamaha
                                                                  Security System setting procedures and
                            EJU43213                              page 38 for Low RPM Mode activation pro-
                            RiDE lever checks (VX / VX Deluxe /
                                                                  cedures.)
                            VX Cruiser / VX Limited)
                                                                  EJU32664
                            Operate the RiDE lever several times to make  Engine shut-off cord (lanyard) check
                            sure that operation is smooth throughout the  Make sure that the engine shut-off cord (lan-
                            whole range. Also, make sure that the RiDE  yard) is not damaged. If the cord is damaged,
                                                                  replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it

                            68

| 69 70 71 72 73 74 75 76 77 78 79 |