Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-85
P. 48

    UF3X12E0.book  Page 42  Friday, May 22, 2020  10:00 AM

                            Watercraft operation

                            (2) Tap the drive control mode indicator on  To operate the watercraft using the drive con-
                                the multifunction information center.  trol mode:
                            (3) If the drive control mode screen is  (1) Release the throttle lever and let the en-
                                locked, the PIN entry screen will be dis-  gine speed return to idle.
                                played. Flick up or down to set each digit  (2) Activate the drive control mode.
                                of the 4-digit PIN, and then tap the “En-  (3) Squeeze  the throttle lever.  The water-
                                ter” button. If the drive control mode  craft will accelerate according to the se-
                                screen is not locked, the screen shown in  lected acceleration setting up to the
                                step 4 will be displayed.            selected maximum watercraft speed set-
                                                                     ting.
                                                                  TIP:
                                         Enter PIN                If the throttle lever is squeezed to a level less
                                    9     9     9     9           than the  selected acceleration  setting, the
                                    0     0     0     0           watercraft will accelerate  according  to the
                                    1     1     1     1           throttle lever operation instead of the select-
                                            Enter                 ed acceleration setting.
                                                                  Selecting the drive control mode settings
                                                                  The drive control mode settings for the max-
                                                                  imum watercraft speed and acceleration are
                            (4) Tap the “ON” button. Once the beeper  saved. In addition, the activation and settings
                                sounds three times and “  ” is displayed  of the drive control mode can be locked to
                                in light blue, the drive control mode is ac-  prevent others from changing them.
                                tivated.                          When the drive control mode is locked, a PIN
                                                                  must be entered to operate the drive control
                                                                  mode screen.
                                       Drive Control              To select the maximum watercraft speed and
                                                                  acceleration settings:
                                      ON          OFF             (1) Perform steps 1–3 in “To activate the
                                                                     drive control mode”.
                                    Settings      Lock            (2) Tap the “Settings” button.
                                                                  (3) Flick up or down to select the maximum
                                                                     watercraft speed setting under “Speed”

                            To deactivate the drive control mode:
                            (1) Perform steps  1–3  in “To activate  the
                                drive control mode”.
                            (2) Tap the “OFF” button. The beeper
                                sounds two times and “  ” is displayed
                                in black when the drive control mode is
                                deactivated.

                            42

| 43 44 45 46 47 48 49 50 51 52 53 |