Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 84 - LIT-18626-12-85
P. 84

    UF3X12E0.book  Page 78  Friday, May 22, 2020  10:00 AM

                            Pre-operation checks

                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]

                                                     MPH

                               0               2    F     100%
                                               3 x100 N
                                13.6V                      N
                                                RPM
                                               4   R
                                                           1
                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.

                              Engine idling speed:
                                1250 ±100 r/min

                            78

| 79 80 81 82 83 84 85 86 87 88 89 |