Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-85
P. 80

    UF3X12E0.book  Page 74  Friday, May 22, 2020  10:00 AM

                            Pre-operation checks

                            EJU40363                              throttle lever returns automatically to its fully
                            Adjustable tilt steering system checks
                            Operate the adjustable tilt steering system  closed (idle) position when released.
                            several times to make sure that operation is
                            smooth throughout the whole range. Also,
                            make sure that the handlebars are securely
                            locked in place. (See page 33 for adjustable
                            tilt steering system operation procedures.)

                                                                  EJU45350
                                                                  Yamaha Security System check
                                                                  Make sure that the Yamaha Security System
                                                                  operates properly. (See page 30 for Yamaha
                                                                  Security System setting procedures.)
                                                                  EJU32664
                                                                  Engine shut-off cord (lanyard) check
                            EJU43213
                            RiDE lever checks                     Make sure that the engine shut-off cord (lan-
                            Operate the RiDE lever several times to make  yard) is not damaged. If the cord is damaged,
                            sure that operation is smooth throughout the  replace it.  WARNING! Never try to repair
                            whole range. Also, make sure that the RiDE  the engine shut-off cord (lanyard) or tie it
                            lever returns automatically to its fully closed  together. The  engine  shut-off cord (lan-
                            position when released.               yard) may not pull free when the operator
                                                                  falls off, allowing the watercraft to contin-
                                                                  ue to run and cause an accident. [EWJ01221]

                            EJU42181
                            Throttle lever checks
                            Operate the throttle lever  several times  to
                                                                  EJU32676
                            make sure that operation is smooth through-  Switch checks
                            out the whole range. Also, make sure that the  ECJ01311
                                                                  Do not run the engine over 4000 r/min on
                                                                  land. Also, do not run the engine for more

                            74

| 75 76 77 78 79 80 81 82 83 84 85 |