Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-12-85
P. 79

    UF3X12E0.book  Page 73  Friday, May 22, 2020  10:00 AM

                                                                    Pre-operation checks

                            shows any other signs of decreased pow-  right and left fully turned positions of the jet
                            er. Loss of battery power may leave you  thrust nozzle.
                            stranded. [EWJ01241]
                             1          2

                              1 Negative (–) battery terminal: Black lead
                              2 Positive (+) battery terminal: Red lead
                            Make sure that the battery is securely held in
                            place.
                            EJU32614
                            Steering system checks
                            Turn the handlebars to the right and left sev-
                            eral times  to make sure that  operation is
                            smooth and  unrestricted throughout  the
                            whole range, and that the free play is not ex-
                            cessive.

                                                                    Difference between fully turned posi-
                                                                    tions of jet thrust nozzle (distances A
                                                                    and B):
                                                                      Maximum 5 mm (0.20 in)
                            Turn the handlebars as far as possible to the
                            right and left to make sure that the jet thrust
                            nozzle moves as the handlebars are turned,
                            and that there is no difference between the

                                                                                                   73

| 74 75 76 77 78 79 80 81 82 83 84 |