Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 87 - LIT-18626-12-85
P. 87

    UF3X12E0.book  Page 81  Friday, May 22, 2020  10:00 AM

                                                                                      Operation

                            (3) Attach the engine shut-off cord (lanyard)  EJU32863
                                                                  Stopping the engine
                                to your left wrist, and then attach the clip
                                                                  Release the throttle lever, and then push the
                                to the engine shut-off switch. (See page
                                                                  engine stop switch (red button) to stop the
                                31 for information on operating the en-
                                                                  engine.  WARNING! You need throttle to
                                gine shut-off switch.) WARNING! Check
                                                                  steer. Shutting the engine off can cause
                                that the engine shut-off cord (lanyard)
                                                                  you to hit an obstacle you are attempting
                                is attached  correctly. If the engine
                                                                  to avoid. A collision could result in severe
                                shut-off cord (lanyard) is not attached
                                                                  injury or death. [EWJ00602]
                                correctly, it may not pull free when the
                                operator falls off, allowing the water-
                                craft to continue to run and cause an
                                accident. [EWJ00582]
                                                     1   2

                                                                  EJU32873
                                                  3               Leaving the watercraft
                                                                  If leaving the watercraft, remove the clip from
                                                                  the  engine shut-off switch  to prevent acci-
                              1 Clip
                                                                  dental starting or unauthorized operation by
                              2 Engine shut-off switch
                                                                  children or others.
                              3 Engine shut-off cord (lanyard)
                            (4) With the throttle lever released, push the
                                start  switch (green  button) to start  the
                                engine. (See page 31 for information on
                                operating the start switch.)

                                                                  EJU43411
                                                                  Operating the watercraft
                                                                  When the throttle lever is squeezed, the “F”
                                                                  (forward) shift indicator will be displayed and
                                                                  the watercraft will move forward. While the
                                                                  “F” (forward) shift indicator is displayed, the
                                                                  watercraft will move forward at trolling speed
                                                                  even if the throttle lever is in the fully closed

                                                                                                   81

| 82 83 84 85 86 87 88 89 90 91 92 |