Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - LIT-18626-12-85
P. 41

    UF3X12E0.book  Page 35  Friday, May 22, 2020  10:00 AM

                                                                      Watercraft operation

                            EJU40014                                 reverse, and the “R” (reverse) shift indi-
                             Watercraft operation functions
                                                                     cator will be displayed.
                            EJU43154
                            Shift system                                              1
                            EWJ01773
                             Make sure that there are no obstacles or
                              people behind you before  shifting  into
                              reverse.
                             Do not touch the reverse gate while the
                              RiDE lever is being operated, otherwise
                              you could be pinched.
                                                                   1 RiDE lever
                             If the RiDE  lever and throttle lever are
                              being operated at the same time, do not
                              release only the RiDE lever. Otherwise,
                              the watercraft  could accelerate more                  1
                              quickly than expected, which may lead
                              to an accident.
                            The RiDE lever and throttle lever can be oper-
                            ated to change the forward or rearward
                                                                                               2
                            movement of the watercraft only when the
                            engine is running.  When the  RiDE  lever is
                            squeezed, the reverse gate lowers and de-  1 Reverse gate
                            flects the water jet being discharged from the  2 Reverse position
                            jet thrust nozzle so that the watercraft moves
                            in reverse or is in neutral. When the throttle le-
                            ver is squeezed, the reverse gate rises and
                            the watercraft moves forward.
                            TIP:                                                           MPH
                             This  model is equipped with a function
                              which limits the engine speed in reverse.  0                      100%
                             When the  engine is started,  the reverse              x100
                                                                     13.6V                      R
                              gate automatically moves to the neutral po-            RPM
                              sition.                                                           1
                            To shift into reverse:                 1 “R” (Reverse position)
                            (1) Release the throttle lever.       To shift into neutral from reverse:
                            (2) Squeeze the  RiDE lever. The reverse  Release the RiDE lever. The reverse gate will
                                gate will lower, the engine speed will in-  automatically return to the  neutral position
                                crease, the watercraft will start moving in

                                                                                                   35

| 36 37 38 39 40 41 42 43 44 45 46 |