Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-85
P. 42

    UF3X12E0.book  Page 36  Friday, May 22, 2020  10:00 AM

                            Watercraft operation

                            and the “N” (neutral) shift indicator will be dis-  To shift into forward:
                            played.                               (1) Release the RiDE lever.
                                                                  (2) Squeeze the throttle lever. The reverse
                                                                     gate  will rise completely, the engine
                                               1
                                                                     speed will increase, the watercraft will
                                                                     start moving forward, and the “F” (for-
                                                                     ward) shift indicator will be displayed.

                                                                          1

                              1 RiDE lever

                                                1

                                                                   1 Throttle lever

                                                         2                    1
                                                                                             2

                              1 Reverse gate
                              2 Neutral position

                                                                   1 Reverse gate
                                                     MPH           2 Forward position

                               0                          100%
                                13.6V           x100       N
                                                RPM
                                                           1                               MPH
                              1 “N” (Neutral position)
                                                                    0                           100%
                            TIP:
                            Although the neutral position helps keep the  13.6V      x100       F
                                                                                     RPM
                            watercraft from moving even when the en-                            1
                            gine is running, some movement may occur.
                                                                   1 “F” (Forward position)

                            36

| 37 38 39 40 41 42 43 44 45 46 47 |