Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 98 - LIT-18626-12-86
P. 98

    UF3V12E0.book  Page 92  Wednesday, June 3, 2020  2:38 PM

                            Care and storage

                                ter flows out continually from  the  jet  (2) Rinse  the engine and engine compart-
                                thrust nozzle.                       ment with a small amount of  water.
                                                                     NOTICE: Do not use high-pressure
                                                                     water when rinsing the engine or en-
                                                                     gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (3) Drain  the water  from the engine com-
                                                                     partment. (See page 66 for information
                                                                     on draining the bilge water.)
                                                                  (4) Wipe  the engine  and engine compart-
                                                                     ment with a dry cloth.
                                                                  (5) Wash down the hull, deck, and jet pump
                            (8) Run the engine at idling speed for about  with fresh water.
                                3 minutes watching the engine condition.  (6) Wipe the hull, deck, and jet pump with a
                                If the  engine stops  while flushing,  turn  dry cloth.
                                the water supply off immediately  and  (7) Wipe  all vinyl and rubber components,
                                perform the procedure again from step 7.  such as the seats and engine compart-
                                NOTICE: Do not supply water to the   ment seals, with a vinyl protectant such
                                cooling water passages when the en-  as Yamaclean Vinyl Dressing™.
                                gine is not running. The water could  (8) To minimize corrosion, spray metallic
                                flow back through the muffler into the  parts of the hull, deck, and engine with a
                                engine, causing severe engine  dam-  rust inhibitor such as Yamalube Silicone
                                                                     Protectant & Lubricant.
                                age. [ECJ00123]
                            (9) Turn the water supply off.        (9) Allow the engine compartment to air dry
                            (10) Discharge the remaining water out of the  completely before installing the seats.
                                cooling  water passages by  alternately  (10) Securely install the seats in their original
                                squeezing and releasing the throttle lever  positions.
                                quickly for 10 to 15 seconds.     EJU41634
                                                                  Battery care
                            (11) Stop the engine.
                                                                  If the watercraft will not be used for more than
                            (12) Remove the garden hose adapter, and
                                                                  a month, remove the battery from the water-
                                then securely install the flushing hose
                                                                  craft, check it, and then store it in a cool, dry
                                connector cap  by tightening  it until it
                                                                  place.
                                stops.                            EWJ00792
                            (13) Securely close the stern  storage com-
                                partment.
                                                                  Battery electrolyte is poisonous and dan-
                            (14) Securely install the removable watertight
                                                                  gerous, causing severe burns, etc. Elec-
                                storage compartment and seats in their
                                                                  trolyte contains sulfuric acid. Avoid
                                original positions.
                                                                  contact with skin, eyes, or clothing.
                            EJU33747
                            Cleaning the watercraft               Antidotes
                            (1) Remove the seats. (See page 54 for seat  External: Flush with water.
                                removal and installation procedures.)
                            92

| 93 94 95 96 97 98 99 100 101 102 103 |